

**HD Analog Day/ Night** **Vari-Focal** **IR** **Box** **Camera**

**CV-CPW101L**

**CV-CPW101LN**

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

**Smart look Day/ Night Vari-Focal Box (Bullet) Camera with IR illuminator**

**illuminator**

**illuminator**

|  |  |  |
| --- | --- | --- |
| Parameter | CV-CPW101L | CV-CPW101LN |
| **Camera** | | |
| Image Sensor | 1/2.9" 1.0 Mega Pixels CMOS | |
| Effective Pixels | 1280 (H) × 720 (V) | |
| Min Illumination | 0.05Lux/ F1.4, 0Lux IR on | |
| Electronic Shutter | 1/50s~1/100,000s | 1/60s~1/100,000s |
| Video Frame Rate | 25fps | 30fps |
| Synchronization | Internal | |
| Day & Night | Auto (ICR)/ Color/ B/W | |
| Max IR Distance | 30m | |
| Digital Noise Reduction | 2D | |
| White Balance | Auto | |
| AGC | Auto | |
| BLC | Auto | |
| **Lens** | | |
| Focal Length | 2.7-12 mm @ Manual/ Fixed Iris | |
| Angular Field of View | H: 35 ~ 93  V: 21 ~ 50 | |
| Lens Type | Φ14 | |
| **Input / Output** | | |
| Video Output | 1 CH BNC HD-CVI video output | |
| **General** | | |
| Power | DC 12V±25% | |
| Power Consumption | 3.2W MAX | |
| Working Temperature | -30℃~+60℃.  Less than 95% RH (no condensation) | |
| Dimensions | Φ90.4 mm × 213 mm | |
| Weight (approx.) | 550g | |
| Installation Mode | Wall mount | |
| External Case | Metal | |



**Specifications**



• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.


• Screw plug ……………………………………... 2 pcs.

**Key Features**

* High-performance CMOS image sensor.
* Support 720p@25fps (PAL)/ 30fps (NTSC).
* Support 75-3 coaxial cable transmission over 800m.
* High speed & long distance real-time transmission.
* Support ICR for day time and night time operation.
* Support auto exposure, auto white balance, auto electronic shutter and auto gain function.
* High image color rendition, vivid image.
* Support manual adjustment of lens zoom and focus.
* Support DC12V power supply.
* IP66 compliance.
* Quick guide……………………....1 pc
* Important safety instruction…….1 pc

**Standard Accessories**

**Appearance**



**Important**

- Safety Precaution: Carefully read the operating instruction manual before using this product.

DISTRIBUTED BY:

* All pictures are simulated.
* Weights and dimensions are approximate.
* Specifications are subject to change without notice.
* These products may be subject to export control regulations.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.