

**4 CH/ 8 CH HD Analog Digital Video Recorder**

**illuminator**

**HD Analog Digital Video Recorder**

**CJ-HDR104**

**CJ-HDR108**

**Specifications**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Model** | | | **CJ-HDR104** | **CJ-HDR108** |
| **Video/ Audio IF** | | | | |
| Video Input | | | 4 CH, BNC | 8 CH, BNC |
| Type | | HDCVI | 720p/ 1080p HDCVI | |
| Analog | NTSC/ PAL | |
| Video Output | | | 1 HDMI, 1 VGA | |
| Audio Input | | | 1 CH , RCA | |
| Audio Output | | | 1 CH , RCA | |
| Two-way Talk | | | Reuse audio input/ output CH 1 | |
| **Display** | | | | |
| Output Resolution | | | 1920×1080, 1280×1024, 1280×720, 1024×768 | |
| Multiscreen Mode | | | 1/4 | 1/4/8/9 |
| Privacy Masking | | | 4 rectangular zones (each camera) | |
| OSD | | | Camera title, Time, Video loss, Camera lock, Motion detection, Recording | |
| **Video/ Audio Format** | | | | |
| Video/ Audio Compression | | | H.264/ G.711 | |
| Record Rate | Main Stream | | 1080P (1~15fps)/ 720P/ 960H/ D1 (1~25/30fps) | |
| Extra Stream | | CIF/ QCIF (1~25/30fps), D1 (1~12/15fps) | |
| Bit Rate | | | 96~4096Kb/s | |
| Record Mode | | | Manual, Schedule (Regular (Continuous), MD), Stop | |
| Record Interval | | | 1~60 min (default: 60 min), Pre-record: 1~30 sec, Post-record: 10~300 sec | |
| **Alarm/ Event** | | | | |
| Trigger Events | | | Recording, PTZ, Tour, Video Push, Email, FTP, Snapshot,  Buzzer & Screen tips | |
| Video Detection | | | Motion Detection, MD Zones: 396 (22×18), Video Loss & Camera Blank | |
| **Playback & Backup** | | | | |
| Sync Playback | | | 1/4 | 1/4/9 |
| Search Mode | | | Time/ Date, MD & Exact search (accurate to second) | |
| Playback Functions | | | Play, Pause, Stop, Rewind, Fast play, Slow play, Next file, Previous file, Next camera, Previous camera, Full screen, Repeat, Shuffle, Backup selection, Digital zoom | |
| Backup Mode | | | USB Device/ Network | |
| **Network** | | | | |
| Network Interface | | | RJ-45 port (10/ 100M) | |
| Network Functions | | | HTTP, IPv4/IPv6, TCP/IP, UPNP, RTSP, UDP, SMTP, NTP, DHCP, DNS, PPPOE, DDNS, FTP, IP Filter, SNMP, P2P | |
| Max. User Access | | | 128 users | |
| Mobile Device | | | iPhone, iPad, Android | |
| **HDD** | | | | |
| Type | | | 1 SATA port, up to 6TB | |
| **External Interface** | | | | |
| USB Interface | | | 2 ports (1 Rear), USB2.0 | |
| RS485 Camera Interface | | | 1 port, For PTZ Control | |
| **General Specifications** | | | | |
| Power Supply | | | DC12V/4A | |
| Power Consumption | | | 10W (without HDD) | |
| Working Environment | | | -10°C~+55°C / 10%~90%RH / 86~106kpa | |
| Dimension(W×D×H) | | | Mini 1U, 325mm×255mm×55mm | |
| Weight | | | 1.5KG (without HDD) | |



• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.


• Screw plug ……………………………………... 2 pcs.

* Up to 4 CH (CJ-HDR104) / 8 CH (CJ-HDR108) real-time recording playback and live view
* H.264 video encode
* HDMI/ VGA simultaneous video output
* Support 1 SATA HDDs up to 6TB, 2 USB (4 CH/ 8 CH)
* Digital Zoom in Live & Playback
* iPhone, iPad, & Android

**Key Features**

* Quick guide…………….………..........1 pc
* Important safety instruction…….1 pc
* CD ………………………………..….........1pc

**Standard Accessories**



**Appearance**

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.


• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.

• Installation Guide ........................................... 1 pc.

• Screw …………………………………………… 2 pcs.

• Screw plug ……………………………………... 2 pcs.



**Important**

- Safety Precaution: Carefully read the operating instruction manual before using this product.

DISTRIBUTED BY:

* All pictures are simulated.
* Weights and dimensions are approximate.
* Specifications are subject to change without notice.
* These products may be subject to export control regulations.